mbformat(1) MB-System 5.0 mbformat(1)

NAME

mbformat − List information about swath sonar data formats supported by the MBIO library.

VERSION

Version 5.0

SYNOPSISmbformat [ −Fformat −Ifile −L −K −V −H] DESCRIPTION

mbformat is a utility which identifies the swath sonar data formats associated with mbio format id’s. If no format id or input filename is specified, mbformat lists all of the currently supported formats along with short descriptions. If a format id is specified using the −F option, then mbformat prints a short description of that format. If a filename is specified using the −I option, then mbformat attempts to identify a valid format id for that file using swath data filename prefix and suffix conventions embedded in MB-System. The program also determines the filename "root", which is the filename minus whatever format-specific prefix or suffix has been recognized. In no prefix or suffix is recognized, then the root is simply the entire filename.

Normally, mbformat prints out a brief description of each identified format. If the −L option is used, mbformat simply prints out the valid format id number, or 0 if a file or format has been specified but no valid id can be identified. If the −K option is used, mbformat will print out the filename "root" followed by the format id number.

AUTHORSHIP

David W. Caress (caress@mbari.org) Monterey Bay Aquarium Research Institute Dale N. Chayes (dale@ldeo.columbia.edu) Lamont-Doherty Earth Observatory

OPTIONS

−F format

Sets the format id to be listed. If no format is given, all of the currently supported formats will be listed. A list of the swath sonar data formats currently supported by MBIO and their identifier values is given in the MBIO manual page.

−H This "help" flag cause the program to print out a description of its operation and then exit immediately.

−I file

Sets the filename to be tested against known filename prefix and suffix conventions in order to identify the format id.

−K Causes the fileroot and the format id to be output. The fileroot is the filename with any format specific suffix removed.

−L Causes the format descriptions to be omitted so that only the MBIO format id numbers are listed.

−V Normally, mbformat only prints out format descriptions. If the −V flag is given, then mbformat works in a "verbose" mode and also outputs the program version being used.

EXAMPLES

Suppose one wishes to identify the swath sonar data format associated with a format id of 11. The following will suffice:

mbformat −F11 and the result will be this output: MBIO data format id: 11 mbformat(1) MB-System 5.0 mbformat(1)

Format name: MBF_SBSIOMRG Informal Description: SIO merge Sea Beam Attributes: Sea Beam, bathymetry, 16 beams, binary, uncentered, SIO.

Suppose one wishes to list all of the currently supported data formats. The following will suffice:

mbformat

Suppose one wants to find out what format is associated with a raw SeaBeam 2112 file named sb199811231045.rec:

mbformat −I sb199811231045.rec This results in the output: MBIO data format id: 41 Format name: MBF_SB2100RW Informal Description: SeaBeam 2100 series vender format Attributes: SeaBeam 2100, bathymetry, amplitude and sidescan, 151 beams and 2000 pixels, ascii with binary sidescan, SeaBeam Instruments.

Using the −K option:

mbformat −K −I sb199811231045.rec will produce the following output: sb199811231045 41 where the format id has been identified as 41 because of the ".rec" file suffix and the fileroot has been identified as "sb199811231045" by removing the suffix. Use of the −L option:

mbformat −L −I sb199811231045.rec will produce output with just format id: 41 SEE ALSO mbsystem(1), mbio(1)

BUGS

No known bugs.