mbm_fmtvel(1) MB-System 5.0 mbm_fmtvel(1)

NAME

mbm_fmtvel − Extract sound velocity info from Hydrosweep data files and create output in tabular format.

VERSION

Version 5.0

SYNOPSIS

mbm_fmtvel [−Fformat −Iinfilename ]

DESCRIPTION mbm_fmtvel is a macro that scans a Hydrosweep swath sonar data file using the program mbhsdump and generates a list in columnar format with time, date, latitude, longitude, C-mean, and C-keel entrys. Comment records (lines) at the top of the output begin with ’#’. The columns are tab-delimited. The only allowed formats are 21 (raw Hydrosweep data) and 24 (L-DEO in-house binary Hydrosweep data).

AUTHORSHIP David W. Caress (caress@mbari.org) Monterey Bay Aquarium Research Institute Dale N. Chayes (dale@ldeo.columbia.edu) Lamont-Doherty Earth Observatory Suzanne H. O’Hara (sohara@ldeo.columbia.edu) Lamont-Doherty Earth Observatory

OPTIONS

−F format

Sets the format for the input swath sonar data using MBIO integer format identifiers. The only allowed formats are 21 (raw Hydrosweep data) and 24 (L-DEO in-house binary Hydrosweep data).

−I infilename

Data file from which the input data will be read.

SEE ALSO

mbsystem(1)

BUGS

Only one output format is currently supported.

MB-System 5.0 7 June 2013 1